

17 POINT FIREPLACE SERVICE/ INSPECTION

* Clean Glass Inside and Out
* Inspect Gasket Seal
* Inspect and Vacuum Logs with Soft Bristle Attachment
* Replace Embers
* Add Lava Rock if Needed
* Test Gas Pressure if Needed
* Inspect Burner Performance
* Clean and Inspect Firebox
* Clean the Outside of the Firebox
* Clean and Inspect Fan
* Vacuum Heat Chamber
* Check for Gas Leaks
* Check Outside Vent
* Check for Carbon Monoxide Leaks
* Check Wall Switch (if applicable)
* Check Burner Ignition
* Run Fireplace to Inspect Flame Quality

Customer:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Address:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Make:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Model:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_